{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["PPin","SPin","BootMode"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"PPin","index":0,"n_rows":180,"n_cols":9,"rows_kept":180,"cut":false,"hidden":false,"merged":[[63,7,64,7],[63,8,64,8],[77,0,77,8],[0,4,0,7],[0,2,0,3],[63,4,64,4],[63,3,64,3],[63,1,64,1],[63,0,64,0]],"flags":["formulas_cached_only"]}
[null,null,"SMA-iMX6",null,"Controller Chip",null,null,null,"SMARC Spec"]
["Pin","Signal","Direction","Termination","Controller","Pin Name","Function","Pin Group","Type/Tolerance"]
["P1","PCAM_PXL_CK1","In","-","iMX6","EIM_D17","CSI1_PIXCLK","EIM0","CMOS / VDD_IO"]
["P2","GND","-","-","-","-","-",null,"-"]
["P3","PCAM_D0","In","-","iMX6","CSI0_DAT12","CSI0_DAT12","CSI","CMOS / VDD_IO"]
["P4","PCAM_D1","In","-","iMX6","CSI0_DAT13","CSI0_DAT13","CSI","CMOS / VDD_IO"]
["P5","PCAM_DE","In","-","iMX6","CSI0_DATA_EN","CSI0_DATA_EN","CSI","CMOS / VDD_IO"]
["P6","PCAM_MCK","Out","-","iMX6","GPIO_0","CLKO","GPIO","CMOS / VDD_IO"]
["P7","PCAM_D2","In","-","iMX6","CSI0_DAT14","CSI0_DAT14","CSI","CMOS / VDD_IO"]
["P8","PCAM_D3","In","-","iMX6","CSI0_DAT15","CSI0_DAT15","CSI","CMOS / VDD_IO"]
["P9","GND","-","-","-","-","-",null,"-"]
["P10","PCAM_D4","In","-","iMX6","CSI0_DAT16","CSI0_DAT16","CSI","CMOS / VDD_IO"]
["P11","PCAM_D5","In","-","iMX6","CSI0_DAT17","CSI0_DAT17","CSI","CMOS / VDD_IO"]
["P12","GND","-","-","-","-","-",null,"-"]
["P13","PCAM_D6","In","-","iMX6","CSI0_DAT18","CSI0_DAT18","CSI","CMOS / VDD_IO"]
["P14","PCAM_D7","In","-","iMX6","CSI0_DAT19","CSI0_DAT19","CSI","CMOS / VDD_IO"]
["P15","GND","-","-","-","-","-",null,"-"]
["P16","PCAM_D8","In","-","-","-","-"]
["P17","PCAM_D9","In","-","-","-","-"]
["P18","GND","-","-","-","-","-",null,"-"]
["P19","GBE_MDI3-","Bi-Dir","-","BCM5481","TRD3M","RGMII",null,"GBE MDI"]
["P20","GBE_MDI3+","Bi-Dir","-","BCM5481","TRD3P","RGMII",null,"GBE MDI"]
["P21","GBE_LINK100#","Out / OD","-","BCM5481","-","-",null,"CMOS 3.3V"]
["P22","GBE_LINK1000#","Out / OD","-","BCM5481","-","-",null,"CMOS 3.3V"]
["P23","GBE_MDI2-","Bi-Dir","-","BCM5481","TRD2M","RGMII",null,"GBE MDI"]
["P24","GBE_MDI2+","Bi-Dir","-","BCM5481","TRD2P","RGMII",null,"GBE MDI"]
["P25","GBE_LINK_ACT#","Out / OD","-","BCM5481","-","-",null,"VDD_IO"]
["P26","GBE_MDI1-","Bi-Dir","-","BCM5481","TRD1M","RGMII",null,"GBE MDI"]
["P27","GBE_MDI1+","Bi-Dir","-","BCM5481","TRD1P","RGMII",null,"GBE MDI"]
["P28","GBE_CTREF","Out","100nF to GND","-","-","-",null,"V-Ref"]
["P29","GBE_MDI0-","Bi-Dir","-","BCM5481","TRD0M","RGMII",null,"GBE MDI"]
["P30","GBE_MDI0+","Bi-Dir","-","BCM5481","TRD0P","RGMII",null,"GBE MDI"]
["P31","SPI0_CS1#","Out","-","iMX6","KEY_COL2","SS1 (SPI1)","GPIO","CMOS / VDD_IO"]
["P32","GND","-","-","-","-","-",null,"-"]
["P33","SDIO_WP","In","W-PU","iMX6","EIM_DA13","GPIO3-13","EIM2+LS","CMOS 3.3V"]
["P34","SDIO_CMD","Bi-Dir","PU-10k","iMX6","SD2_CMD","SD2_CMD","SD2","CMOS 3.3V"]
["P35","SDIO_CD#","In","PU-10k","iMX6","EIM_DA14","GPIO3-14","EIM2+LS","CMOS 3.3V"]
["P36","SDIO_CK","Out","-","iMX6","SD2_CLK","SD2_CLK","SD2","CMOS 3.3V"]
["P37","SDIO_PWR_EN","Out","-","iMX6","ENET_CRS_DV","GPIO1-25","ENET","CMOS 3.3V"]
["P38","GND","-","-","-","-","-",null,"-"]
["P39","SDIO_D0","Bi-Dir","-","iMX6","SD2_DAT0","SD2_DAT0","SD2","CMOS 3.3V"]
["P40","SDIO_D1","Bi-Dir","-","iMX6","SD2_DAT1","SD2_DAT1","SD2","CMOS 3.3V"]
["P41","SDIO_D2","Bi-Dir","-","iMX6","SD2_DAT2","SD2_DAT2","SD2","CMOS 3.3V"]
["P42","SDIO_D3","Bi-Dir","PD-300k","iMX6","SD2_DAT3","SD2_DAT3","SD2","CMOS 3.3V"]
["P43","SPI0_CS0#","Out","-","iMX6","KEY_ROW1","SS0 (SPI1)","GPIO","CMOS / VDD_IO"]
["P44","SPI0_CK","Out","Serial 20R","iMX6","KEY_COL0","SCLK (SPI1)","GPIO","CMOS / VDD_IO"]
["P45","SPI0_DIN","In","Serial 0R","iMX6","KEY_COL1","MISO (SPI1)","GPIO","CMOS / VDD_IO"]
["P46","SPI0_DO","Out","Serial 20R","iMX6","KEY_ROW0","MOSI (SPI1)","GPIO","CMOS / VDD_IO"]
["P47","GND","-","-","-","-","-",null,"-"]
["P48","SATA_TX+","Out","Serial 10nF","iMX6","SATA_TXP","SATA_TXP","SATA","SATA"]
["P49","SATA_TX-","Out","Serial 10nF","iMX6","SATA_TXM","SATA_TXM","SATA","SATA"]
["P50","GND","-","-","-","-","-",null,"-"]
["P51","SATA_RX+","In","-","iMX6","SATA_RXP","SATA_RXP","SATA","SATA"]
["P52","SATA_RX-","In","-","iMX6","SATA_RXM","SATA_RXM","SATA","SATA"]
["P53","GND","-","-","-","-","-",null,"-"]
["P54","SPI1_CS0#","Out","-","iMX6","EIM_RW","SS0 (SPI2)","EIM1","CMOS / VDD_IO"]
["P55","SPI1_CS1#","Out","-","iMX6","EIM_LBA","SS1 (SPI2)","EIM1","CMOS / VDD_IO"]
["P56","SPI1_CK","Out","-","iMX6","EIM_CS0","SCLK (SPI2)","EIM1","CMOS / VDD_IO"]
["P57","SPI1_DIN","In","-","iMX6","EIM_OE","MISO (SPI2)","EIM1","CMOS / VDD_IO"]
["P58","SPI1_DO","Out","-","iMX6","EIM_CS1","MOSI (SPI2)","EIM1","CMOS / VDD_IO"]
["P59","GND","-","-","-","-","-",null,"-"]
["P60","USB0+","Bi-Dir","-","iMX6","USB_OTG_DP","USB_OTG_DP","USB","USB"]
["P61","USB0-","Bi-Dir","-","iMX6","USB_OTG_DN","USB_OTG_DN","USB","USB"]
["P62","USB0_EN_OC#","Bi-Dir / OD","PU-10k","iMX6","EIM_D22","OTG_PWR","EIM0\n+Level shift (LS)","CMOS 3.3V"]
[null,null,"In",null,null,"EIM_D21","OTG_OC"]
["P63","USB0_VBUS_DET","In","-","Switch-3.3V","-","-",null,"VBUS 5.0V"]
["P64","USB0_OTG_ID","In","-","iMX6","ENET_RX_ER","OTG_ID","ENET","CMOS 3.3V"]
["P65","USB1+","Bi-Dir","-","iMX6","USB_H1_DP","USB_H1_DP","USB","USB"]
["P66","USB1-","Bi-Dir","-","iMX6","USB_H1_DN","USB_H1_DN","USB","USB"]
["P67","USB1_EN_OC#","In","PU-10k","iMX6","EIM_D30","H1_OC","EIM0","CMOS 3.3V"]
["P68","GND","-","-","-","-","-",null,"-"]
["P69","USB2+","Bi-Dir","-","-","-","-",null,"USB"]
["P70","USB2-","Bi-Dir","-","-","-","-",null,"USB"]
["P71","USB2_EN_OC#","In","PU-10k","-","-","-",null,"CMOS 3.3V"]
["P72","PCIE_C_PRSNT#","In","PU-36k","iMX6","EIM_DA8","GPIO3-8","EIM2+LS","CMOS 3.3V"]
["P73","PCIE_B_PRSNT#","In","PU-36k","iMX6","EIM_DA9","GPIO3-9","EIM2+LS","CMOS 3.3V"]
["P74","PCIE_A_PRSNT#","In","PU-36k","iMX6","ENET_RXD0","GPIO1-27","ENET","CMOS 3.3V"]
["Key"]
["P75","PCIE_A_RST#","Out","-","iMX6","GPIO_19","GPIO4-5","GPIO+LS","CMOS 3.3V"]
["P76","PCIE_C_CKREQ#","In","PU-36k","iMX6","ENET_TXD0","GPIO1-30","ENET","CMOS 3.3V"]
["P77","PCIE_B_CKREQ#","In","PU-36k","iMX6","ENET_TXD1","GPIO1-29","ENET","CMOS 3.3V"]
["P78","PCIE_A_CKREQ#","In","PU-36k","iMX6","ENET_TX_EN","GPIO1-28","ENET","CMOS 3.3V"]
["P79","GND","-","-","-","-","-",null,"-"]
["P80","PCIE_C_REFCK+","Out","-","PEX8605","PEX_REFCLK_OUTP3","-",null,"LVDS PCIe"]
["P81","PCIE_C_REFCK-","Out","-","PEX8605","PEX_REFCLK_OUTN3","-",null,"LVDS PCIe"]
["P82","GND","-","-","-","-","-",null,"-"]
["P83","PCIE_A_REFCK+","Out","-","PEX8605","PEX_REFCLK_OUTP1","-",null,"LVDS PCIe"]
["P84","PCIE_A_REFCK-","Out","-","PEX8605","PEX_REFCLK_OUTN1","-",null,"LVDS PCIe"]
["P85","GND","-","-","-","-","-",null,"-"]
["P86","PCIE_A_RX+","In","Serial-0R","PEX8605","PEX_PERP1","-",null,"LVDS PCIe"]
["P87","PCIE_A_RX-","In","Serial-0R","PEX8605","PEX_PERN1","-",null,"LVDS PCIe"]
["P88","GND","-","-","-","-","-",null,"-"]
["P89","PCIE_A_TX+","Out","Seriell-100n","PEX8605","PEX_PETP1","-",null,"LVDS PCIe"]
["P90","PCIE_A_TX-","Out","Seriell-100n","PEX8605","PEX_PETN1","-",null,"LVDS PCIe"]
["P91","GND","-","-","-","-","-",null,"-"]
["P92","HDMI_D2+","Out","-","iMX6","HDMI_D2P","HDMI_D2P","HDMI","TMDS"]
["P93","HDMI_D2-","Out","-","iMX6","HDMI_D2M","HDMI_D2M","HDMI","TMDS"]
["P94","GND","-","-","-","-","-",null,"-"]
["P95","HDMI_D1+","Out","-","iMX6","HDMI_D1P","HDMI_D1P","HDMI","TMDS"]
["P96","HDMI_D1-","Out","-","iMX6","HDMI_D1M","HDMI_D1M","HDMI","TMDS"]
["P97","GND","-","-","-","-","-",null,"-"]
["P98","HDMI_D0+","Out","-","iMX6","HDMI_D0P","HDMI_D0P","HDMI","TMDS"]
["P99","HDMI_D0-","Out","-","iMX6","HDMI_D0M","HDMI_D0M","HDMI","TMDS"]
["P100","GND","-","-","-","-","-",null,"-"]
["P101","HDMI_CK+","Out","-","iMX6","HDMI_CLKP","HDMI_CLKP","HDMI","TMDS"]
["P102","HDMI_CK-","Out","-","iMX6","HDMI_CLKM","HDMI_CLKM","HDMI","TMDS"]
["P103","GND","-","-","-","-","-",null,"-"]
["P104","HDMI_HPD","In","PU-39k","iMX6","HDMI_HPD","HDMI_HPD","HDMI+LS","CMOS / VDD_IO"]
["P105","HDMI_CTRL_CK","Out","PU-2k2","iMX6","GPIO_3","SCL (I2C3)","GPIO","CMOS / VDD_IO"]
["P106","HDMI_CTRL_DAT","Bi-Dir","PU-2k2","iMX6","GPIO_6","SDA (I2C3)","GPIO","CMOS / VDD_IO"]
["P107","HDMI_CEC","Bi-Dir","PU-39k","iMX6","HDMI_DDCCEC","HDMI_DDCCEC","HDMI+LS","CMOS / VDD_IO"]
["P108","GPIO0","Bi-Dir","-","iMX6","SD1_DAT0","GPIO1-16","SD1","CMOS / VDD_IO"]
["P109","GPIO1","Bi-Dir","-","iMX6","SD1_DAT1","GPIO1-17","SD1","CMOS / VDD_IO"]
["P110","GPIO2","Bi-Dir","-","iMX6","NANDF_D3","GPIO2-3","CSI","CMOS / VDD_IO"]
["P111","GPIO3","Bi-Dir","-","iMX6","NANDF_D4","GPIO2-4","CSI","CMOS / VDD_IO"]
["P112","GPIO4","Bi-Dir","-","iMX6","NANDF_D0","GPIO2-0","EIM0","CMOS / VDD_IO"]
["P113","GPIO5/PWM_OUT","Bi-Dir","-","iMX6","SD1_CMD","GPIO1-18","EIM0","CMOS / VDD_IO"]
["P114","GPIO6","Bi-Dir","-","iMX6","EIM_BCLK","GPIO6-31","EIM2","CMOS / VDD_IO"]
["P115","GPIO7","Bi-Dir","-","iMX6","NANDF_D1","GPIO5-0","EIM2","CMOS / VDD_IO"]
["P116","GPIO8","Bi-Dir","-","iMX6","NANDF_D2","GPIO2-28","EIM2","CMOS / VDD_IO"]
["P117","GPIO9","Bi-Dir","-","iMX6","EIM_D16","GPIO3-16","EIM0","CMOS / VDD_IO"]
["P118","GPIO10/SER1_CTS","Bi-Dir","-","iMX6","EIM_D28","GPIO3-28 / uart2-CTS","EIM0","CMOS / VDD_IO"]
["P119","GPIO11/SER1_RTS","Bi-Dir","-","iMX6","EIM_D29","GPIO3-29 / uart2-RTS","EIM0","CMOS / VDD_IO"]
["P120","GND","-","-","-","-","-",null,"-"]
["P121","I2C_PM_CK","Out","-","iMX6","KEY_COL3","SCL (I2C2)","GPIO","CMOS 1.8V"]
["P122","I2C_PM_DAT","Bi-Dir","-","iMX6","KEY_ROW3","SDA (I2C2)","GPIO","CMOS 1.8V"]
["P123","BOOT_SEL0#","In","W-PU","FPGA","-","-",null,"CMOS / VDD_IO"]
["P124","BOOT_SEL1#","In","W-PU","FPGA","-","-",null,"CMOS / VDD_IO"]
["P125","BOOT_SEL2#","In","W-PU","FPGA","-","-",null,"CMOS / VDD_IO"]
["P126","RESET_OUT#","Out-OD","-","FPGA","-","-",null,"CMOS / VDD_IO"]
["P127","RESET_IN#","In","W-PU","FPGA","-","-",null,"CMOS / VDD_IO"]
["P128","POWER_BTN# (*1)","In","W-PU","FPGA","-","-",null,"CMOS / VDD_SNVS (3.3V)"]
["P129","SER0_TX","Out","-","iMX6","CSI0_DAT10","TXD (UART1)","CSI","CMOS / VDD_IO"]
["P130","SER0_RX","In","W-PU","iMX6","CSI0_DAT11","RXD (UART1)","CSI","CMOS / VDD_IO"]
["P131","SER0_RTS#","Out","-","iMX6","EIM_D20","RTS (UART1)","EMI0","CMOS / VDD_IO"]
["P132","SER0_CTS#","In","W-PU","iMX6","EIM_D19","CTS (UART1)","EMI0","CMOS / VDD_IO"]
["P133","GND","-","-","-","-","-",null,"-"]
["P134","SER1_TX","Out","-","iMX6","EIM_D26","TXD (UART2)","EMI0","CMOS / VDD_IO"]
["P135","SER1_RX","In","W-PU","iMX6","EIM_D27","RXD (UART2)","EMI0","CMOS / VDD_IO"]
["P136","SER2_TX","Out","-","iMX6","EIM_D24","TXD (UART3)","EMI0","CMOS / VDD_IO"]
["P137","SER2_RX","In","W-PU","iMX6","EIM_D25","RXD (UART3)","EMI0","CMOS / VDD_IO"]
["P138","SER2_RTS#","Out","-","iMX6","EIM_D31","RTS (UART3)","EMI0","CMOS / VDD_IO"]
["P139","SER2_CTS#","In","W-PU","iMX6","EIM_D23","CTS (UART3)","EMI0","CMOS / VDD_IO"]
["P140","SER3_TX","Out","-","iMX6","CSI0_DAT12","TXD (UART4)","CSI","CMOS / VDD_IO"]
["P141","SER3_RX","In","W-PU","iMX6","CSI0_DAT13","RXD (UART4)","CSI","CMOS / VDD_IO"]
["P142","GND","-","-","-","-","-",null,"-"]
["P143","CAN0_TX","Out","-","iMX6","GPIO_7","TXCAN (CAN1)","GPIO","CMOS / VDD_IO"]
["P144","CAN0_RX","In","W-PU","iMX6","GPIO_8","RXCAN (CAN1)","GPIO","CMOS / VDD_IO"]
["P145","CAN1_TX","Out","-","iMX6","KEY_COL4","TXCAN (CAN2)","GPIO","CMOS / VDD_IO"]
["P146","CAN1_RX","In","W-PU","iMX6","KEY_ROW4","RXCAN (CAN2)","GPIO","CMOS / VDD_IO"]
["P147","VDD_IN","PWR_IN","-","-","-","-",null,"-"]
["P148","VDD_IN","PWR_IN","-","-","-","-",null,"-"]
["P149","VDD_IN","PWR_IN","-","-","-","-",null,"-"]
["P150","VDD_IN","PWR_IN","-","-","-","-",null,"-"]
["P151","VDD_IN","PWR_IN","-","-","-","-",null,"-"]
["P152","VDD_IN","PWR_IN","-","-","-","-",null,"-"]
["P153","VDD_IN","PWR_IN","-","-","-","-",null,"-"]
["P154","VDD_IN","PWR_IN","-","-","-","-",null,"-"]
["P155","VDD_IN","PWR_IN","-","-","-","-",null,"-"]
["P156","VDD_IN","PWR_IN","-","-","-","-",null,"-"]
[]
[null,"W-PU is PU-100k"]
[null,"ENET and SD2 pin group 為 3.3V"]
[null,"重覆使用到 iMX6 Pins, Carrier board 必須避免同時使用."]
["P3","PCAM_D0","In","-","iMX6","CSI0_DAT12","CSI0_DAT12","CSI","CMOS / VDD_IO"]
["P4","PCAM_D1","In","-","iMX6","CSI0_DAT13","CSI0_DAT13","CSI","CMOS / VDD_IO"]
["P140","SER3_TX","Out","-","iMX6","CSI0_DAT12","TXD (UART4)","CSI","CMOS / VDD_IO"]
["P141","SER3_RX","In","W-PU","iMX6","CSI0_DAT13","RXD (UART4)","CSI","CMOS / VDD_IO"]
["P77","PCIE_B_CKREQ#","In","PU-36k","iMX6","ENET_TXD1","GPIO1-29","ENET","CMOS 3.3V"]
["S17","AFB0_OUT(MLB_CLK)","Out","-","iMX6","GPIO_3","TBD","ENET+LS","CMOS / VDD_IO"]
["P106","HDMI_CTRL_DAT","Bi-Dir","PU-2k2","iMX6","GPIO_6","SDA (I2C3)","GPIO","CMOS / VDD_IO"]
["S19","AFB2_OUT(MLB_SIG)","Out","PU-2k2","iMX6","GPIO_6","TBD","GPIO","CMOS / VDD_IO"]
[]
[null,"+LS","為訊號有加 Level shift IC"]
[null,null,"Signal transfered by CPLD, will tri-state during iMX6 reset, drive to iMX6 after the end of iMX6 reset."]
["(*1)","For power up during power off, do not follow SMARC spec."]
[]
[null,"iMX6 Free Pins"]
[{"$nulls":5},"ENET_RXD1","Unused","ENET"]
[{"$nulls":5},"EIM_EB1","Can not use","EIM2"]

{"sheet":"SPin","index":1,"n_rows":212,"n_cols":9,"rows_kept":212,"cut":false,"hidden":false,"merged":[[162,0,162,8],[0,2,0,3],[0,4,0,7],[77,0,77,8]],"flags":["formulas_cached_only"]}
[null,null,"SMA-iMX6",null,"Controller Chip",null,null,null,"SMARC Spec"]
["Pin","Signal","Direction","Termination","Controller","Pin Name","Function","Pin Group","Type/Tolerance"]
["S1","PCAM_VSYNC","In","-","iMX6","CSI0_VSYNC","CSI0_VSYNC","CSI","CMOS / VDD_IO"]
["S2","PCAM_HSYNC","In","-","iMX6","CSI0_MCLK","CSI0_HSYNC","CSI","CMOS / VDD_IO"]
["S3","GND","-","-","-","-","-",null,"-"]
["S4","PCAM_PXL_CK0","In","-","iMX6","CSI0_PIXCLK","CSI0_PIXCLK","CSI","CMOS / VDD_IO"]
["S5","I2C_CAM_CK","Out","PU-2k2","iMX6","KEY_COL3","SCL (I2C2)","GPIO","CMOS / VDD_IO"]
["S6","CAM_MCK","Out","-","iMX6","GPIO_0","CLKO","GPIO","CMOS / VDD_IO"]
["S7","I2C_CAM_DAT","Bi-Dir","PU-2k2","iMX6","KEY_ROW3","SDA (I2C2)","GPIO","CMOS / VDD_IO"]
["S8","CSI0_CK+","In","-","iMX6","CSI_CLK0P","CSI_CLK0P","MIPI","LVDS D-PHY"]
["S9","CSI0_CK-","In","-","iMX6","CSI_CLK0M","CSI_CLK0M","MIPI","LVDS D-PHY"]
["S10","GND","-","-","-","-","-",null,"-"]
["S11","CSI0_D0+","In","-","iMX6","CSI_D0P","CSI_D0P","MIPI","LVDS D-PHY"]
["S12","CSI0_D0-","In","-","iMX6","CSI_D0M","CSI_D0M","MIPI","LVDS D-PHY"]
["S13","GND","-","-","-","-","-",null,"-"]
["S14","CSI0_D1+","In","-","iMX6","CSI_D1P","CSI_D1P","MIPI","LVDS D-PHY"]
["S15","CSI0_D1-","In","-","iMX6","CSI_D1M","CSI_D1M","MIPI","LVDS D-PHY"]
["S16","GND","-","-","-","-","-",null,"-"]
["S17","AFB0_OUT(MLB_CLK)","Out","-","iMX6","ENET_TXD1","TBD","ENET+LS","CMOS / VDD_IO"]
["S18","AFB1_OUT(MLB_DAT)","Bi-Dir","-","iMX6","GPIO_2","TBD","GPIO","CMOS / VDD_IO"]
["S19","AFB2_OUT(MLB_SIG)","Out","PU-2k2","iMX6","GPIO_6","TBD","GPIO","CMOS / VDD_IO"]
["S20","AFB3_IN","In","-","-","-","-",null,"CMOS / VDD_IO"]
["S21","AFB4_IN","In","-","-","-","-",null,"CMOS / VDD_IO"]
["S22","AFB5_IN","In","-","-","-","-",null,"CMOS / VDD_IO"]
["S23","AFB6_PTIO","Bi-Dir","-","iMX6","GPIO_9","GPIO1-9","GPIO","CMOS / VDD_IO protected"]
["S24","AFB7_PTIO","Bi-Dir","-","iMX6","EIM_D18","GPIO3-18","GPIO","CMOS / VDD_IO protected"]
["S25","GND","-","-","-","-","-",null,"-"]
["S26","SDMMC_D0","Bi-Dir","-","iMX6","SD3_DAT0","DAT0","SD3","CMOS / VDD_IO"]
["S27","SDMMC_D1","Bi-Dir","-","iMX6","SD3_DAT1","DAT1","SD3","CMOS / VDD_IO"]
["S28","SDMMC_D2","Bi-Dir","-","iMX6","SD3_DAT2","DAT2","SD3","CMOS / VDD_IO"]
["S29","SDMMC_D3","Bi-Dir","-","iMX6","SD3_DAT3","DAT3","SD3","CMOS / VDD_IO"]
["S30","SDMMC_D4","Bi-Dir","-","iMX6","SD3_DAT4","DAT4","SD3","CMOS / VDD_IO"]
["S31","SDMMC_D5","Bi-Dir","-","iMX6","SD3_DAT5","DAT5","SD3","CMOS / VDD_IO"]
["S32","SDMMC_D6","Bi-Dir","-","iMX6","SD3_DAT6","DAT6","SD3","CMOS / VDD_IO"]
["S33","SDMMC_D7","Bi-Dir","-","iMX6","SD3_DAT7","DAT7","SD3","CMOS / VDD_IO"]
["S34","GND","-","-","-","-","-",null,"-"]
["S35","SDMMC_CK","Out","-","iMX6","SD3_CLK","CLK","SD3","CMOS / VDD_IO"]
["S36","SDMMC_CMD","Bi-Dir","PU-10k","iMX6","SD3_CMD","CMD","SD3","CMOS / VDD_IO"]
["S37","SDMMC_RST#","Out",null,"iMX6","SD3_RST","RST","SD3","CMOS / VDD_IO"]
["S38","AUDIO_MCK","Out","-","iMX6","GPIO_0","CLKO","GPIO","CMOS / VDD_IO"]
["S39","I2S0_LRCK","Bi-Dir","-","iMX6","CSI0_DAT6","AUD3_TXFS","CSI","CMOS / VDD_IO"]
["S40","I2S0_SDOUT","Out","-","iMX6","CSI0_DAT5","AUD3_TXD","CSI","CMOS / VDD_IO"]
["S41","I2S0_SDIN","In","-","iMX6","CSI0_DAT7","AUD3_RXD","CSI","CMOS / VDD_IO"]
["S42","I2S0_CK","Bi-Dir","-","iMX6","CSI0_DAT4","AUD3_TXC","CSI","CMOS / VDD_IO"]
["S43","I2S1_LRCK","Bi-Dir","-","iMX6","DISP0_DAT22","AUD4_TXFS","LCD","CMOS / VDD_IO"]
["S44","I2S1_SDOUT","Out","-","iMX6","DISP0_DAT21","AUD4_TXD","LCD","CMOS / VDD_IO"]
["S45","I2S1_SDIN","In","-","iMX6","DISP0_DAT23","AUD4_RXD","LCD","CMOS / VDD_IO"]
["S46","I2S1_CK","Bi-Dir","-","iMX6","DISP0_DAT20","AUD4_TXC","LCD","CMOS / VDD_IO"]
["S47","GND","-","-","-","-","-",null,"-"]
["S48","I2C_GP_CK","Out","PU-2k2","iMX6","CSI0_DAT9","SCL (I2C1)","CSI","CMOS / VDD_IO"]
["S49","I2C_GP_DAT","Bi-Dir","PU-2k2","iMX6","CSI0_DAT8","SDA (I2C1)","CSI","CMOS / VDD_IO"]
["S50","I2S2_LRCK","Bi-Dir","-","iMX6","DISP0_DAT18","AUD5_TXFS","LCD","CMOS / VDD_IO"]
["S51","I2S2_SDOUT","Out","-","iMX6","DISP0_DAT17","AUD5_TXD","LCD","CMOS / VDD_IO"]
["S52","I2S2_SDIN","In","-","iMX6","DISP0_DAT19","AUD5_RXD","LCD","CMOS / VDD_IO"]
["S53","I2S2_CK","Bi-Dir","-","iMX6","DISP0_DAT16","AUD5_TXC","LCD","CMOS / VDD_IO"]
["S54","SATA_ACT#","Out","-","-","-","-",null,"CMOS 3.3V"]
["S55","AFB8_PTIO","Out","-","iMX6","NANDF_D7","GPIO2-7","NANDF","CMOS / VDD_IO"]
["S56","AFB9_PTIO","Out","-","iMX6","NANDF_D6","GPIO2-6","NANDF","CMOS / VDD_IO"]
["S57","PCAM_ON_CSI0#","type","float","-","-","-",null,"-"]
["S58","PCAM_ON_CSI1#","type","GND","-","-","-",null,"-"]
["S59","SPDIF_OUT","Out","PU-2k2","iMX6","GPIO_17","OUT1 (SPDIF)","GPIO","CMOS / VDD_IO"]
["S60","SPDIF_IN (*1)","In","PU-2k2","iMX6","GPIO_16","IN1 (SPDIF)","GPIO","CMOS / VDD_IO"]
["S61","GND","-","-","-","-","-",null,"-"]
["S62","AFB_DIFF0+","Bi-Dir","-","-","-","-",null,"LVDS_AFB"]
["S63","AFB_DIFF0-","Bi-Dir","-","-","-","-",null,"LVDS_AFB"]
["S64","GND","-","-","-","-","-",null,"-"]
["S65","AFB_DIFF1+","Bi-Dir","-","-","-","-",null,"LVDS_AFB"]
["S66","AFB_DIFF1-","Bi-Dir","-","-","-","-",null,"LVDS_AFB"]
["S67","GND","-","-","-","-","-",null,"-"]
["S68","AFB_DIFF2+","Bi-Dir","-","iMX6","MLB_CP","MLB_CP","MLB","LVDS_AFB"]
["S69","AFB_DIFF2-","Bi-Dir","-","iMX6","MLB_CN","MLB_CN","MLB","LVDS_AFB"]
["S70","GND","-","-","-","-","-",null,"-"]
["S71","AFB_DIFF3+","Bi-Dir","-","iMX6","MLB_DP","MLB_DP","MLB","LVDS_AFB"]
["S72","AFB_DIFF3-","Bi-Dir","-","iMX6","MLB_DN","MLB_DN","MLB","LVDS_AFB"]
["S73","GND","-","-","-","-","-",null,"-"]
["S74","AFB_DIFF4+","Bi-Dir","-","iMX6","MLB_SP","MLB_SP","MLB","LVDS_AFB"]
["S75","AFB_DIFF4-","Bi-Dir","-","iMX6","MLB_SN","MLB_SN","MLB","LVDS_AFB"]
["Key"]
["S76","PCIE_B_RST#","Out","-","iMX6","GPIO_19","GPIO4-5","GPIO+LS","CMOS 3.3V"]
["S77","PCIE_C_RST#","Out","-","iMX6","GPIO_19","GPIO4-5","GPIO+LS","CMOS 3.3V"]
["S78","PCIE_C_RX+","In","-","PEX8605","PEX_PERP3","-",null,"LVDS PCIe"]
["S79","PCIE_C_RX-","In","-","PEX8605","PEX_PERN3","-",null,"LVDS PCIe"]
["S80","GND","-","-","-","-","-",null,"-"]
["S81","PCIE_C_TX+","Out","Seriell-100n","PEX8605","PEX_PETP3","-",null,"LVDS PCIe"]
["S82","PCIE_C_TX-","Out","Seriell-100n","PEX8605","PEX_PETN3","-",null,"LVDS PCIe"]
["S83","GND","-","-","-","-","-",null,"-"]
["S84","PCIE_B_REFCK+","Out","-","PEX8605","PEX_REFCLK_OUTP2","-",null,"LVDS PCIe"]
["S85","PCIE_B_REFCK-","Out","-","PEX8605","PEX_REFCLK_OUTN2","-",null,"LVDS PCIe"]
["S86","GND","-","-","-","-","-",null,"-"]
["S87","PCIE_B_RX+","In","Serial-0R","PEX8605","PEX_PERP2","-",null,"LVDS PCIe"]
["S88","PCIE_B_RX-","In","Serial-0R","PEX8605","PEX_PERN2","-",null,"LVDS PCIe"]
["S89","GND","-","-","-","-","-",null,"-"]
["S90","PCIE_B_TX+","Out","Seriell-100n","PEX8605","PEX_PETP2","-",null,"LVDS PCIe"]
["S91","PCIE_B_TX-","Out","Seriell-100n","PEX8605","PEX_PETN2","-",null,"LVDS PCIe"]
["S92","GND","-","-","-","-","-",null,"-"]
["S93","LCD_D0","Out","-","iMX6","DISP0_DAT0","LCD_D0","LCD","CMOS / VDD_IO"]
["S94","LCD_D1","Out","-","iMX6","DISP0_DAT1","LCD_D1","LCD","CMOS / VDD_IO"]
["S95","LCD_D2","Out","-","iMX6","DISP0_DAT2","LCD_D2","LCD","CMOS / VDD_IO"]
["S96","LCD_D3","Out","-","iMX6","DISP0_DAT3","LCD_D3","LCD","CMOS / VDD_IO"]
["S97","LCD_D4","Out","-","iMX6","DISP0_DAT4","LCD_D4","LCD","CMOS / VDD_IO"]
["S98","LCD_D5","Out","-","iMX6","DISP0_DAT5","LCD_D5","LCD","CMOS / VDD_IO"]
["S99","LCD_D6","Out","-","iMX6","DISP0_DAT6","LCD_D6","LCD","CMOS / VDD_IO"]
["S100","LCD_D7","Out","-","iMX6","DISP0_DAT7","LCD_D7","LCD","CMOS / VDD_IO"]
["S101","GND","-","-","-","-","-",null,"-"]
["S102","LCD_D8","Out","-","iMX6","DISP0_DAT8","LCD_D8","LCD","CMOS / VDD_IO"]
["S103","LCD_D9","Out","-","iMX6","DISP0_DAT9","LCD_D9","LCD","CMOS / VDD_IO"]
["S104","LCD_D10","Out","-","iMX6","DISP0_DAT10","LCD_D10","LCD","CMOS / VDD_IO"]
["S105","LCD_D11","Out","-","iMX6","DISP0_DAT11","LCD_D11","LCD","CMOS / VDD_IO"]
["S106","LCD_D12","Out","-","iMX6","DISP0_DAT12","LCD_D12","LCD","CMOS / VDD_IO"]
["S107","LCD_D13","Out","-","iMX6","DISP0_DAT13","LCD_D13","LCD","CMOS / VDD_IO"]
["S108","LCD_D14","Out","-","iMX6","DISP0_DAT14","LCD_D14","LCD","CMOS / VDD_IO"]
["S109","LCD_D15","Out","-","iMX6","DISP0_DAT15","LCD_D15","LCD","CMOS / VDD_IO"]
["S110","GND","-","-","-","-","-",null,"-"]
["S111","LCD_D16","Out","-","iMX6","DISP0_DAT16 (I2S2)","LCD_D16","LCD","CMOS / VDD_IO"]
["S112","LCD_D17","Out","-","iMX6","DISP0_DAT17 (I2S2)","LCD_D17","LCD","CMOS / VDD_IO"]
["S113","LCD_D18","Out","-","iMX6","DISP0_DAT18 (I2S2)","LCD_D18","LCD","CMOS / VDD_IO"]
["S114","LCD_D19","Out","-","iMX6","DISP0_DAT19 (I2S2)","LCD_D19","LCD","CMOS / VDD_IO"]
["S115","LCD_D20","Out","-","iMX6","DISP0_DAT20 (I2S1)","LCD_D20","LCD","CMOS / VDD_IO"]
["S116","LCD_D21","Out","-","iMX6","DISP0_DAT21 (I2S1)","LCD_D21","LCD","CMOS / VDD_IO"]
["S117","LCD_D22","Out","-","iMX6","DISP0_DAT22 (I2S1)","LCD_D22","LCD","CMOS / VDD_IO"]
["S118","LCD_D23","Out","-","iMX6","DISP0_DAT23 (I2S1)","LCD_D23","LCD","CMOS / VDD_IO"]
["S119","GND","-","-","-","-","-",null,"-"]
["S120","LCD_DE","Out","PD-10k","iMX6","DI0_PIN15","DI0_PIN15","LCD","CMOS / VDD_IO"]
["S121","LCD_VS","Out","-","iMX6","DI0_PIN3","DI0_PIN3","LCD","CMOS / VDD_IO"]
["S122","LCD_HS","Out","-","iMX6","DI0_PIN2","DI0_PIN2","LCD","CMOS / VDD_IO"]
["S123","LCD_PCK","Out","-","iMX6","DI0_DISP_CLK","DI0_DISP_CLK","LCD","CMOS / VDD_IO"]
["S124","GND","-","-","-","-","-",null,"-"]
["S125","LVDS0TX+","Out","-","iMX6","LVDS0_TX0_P","LVDS0_TX0_P","LVDS","LVDS LCD"]
["S126","LVDS0TX-","Out","-","iMX6","LVDS0_TX0_N","LVDS0_TX0_N","LVDS","LVDS LCD"]
["S127","LCD_BKLT_EN","Out","-","iMX6","EIM_DA0","GPIO3-0","EIM2","CMOS / VDD_IO"]
["S128","LVDS0TX1+","Out","-","iMX6","LVDS0_TX1_P","LVDS0_TX1_P","LVDS","LVDS LCD"]
["S129","LVDS0TX1-","Out","-","iMX6","LVDS0_TX1_N","LVDS0_TX1_N","LVDS","LVDS LCD"]
["S130","GND","-","-","-","-","-",null,"-"]
["S131","LVDS0TX2+","Out","-","iMX6","LVDS0_TX2_P","LVDS0_TX2_P","LVDS","LVDS LCD"]
["S132","LVDS0TX2-","Out","-","iMX6","LVDS0_TX2_N","LVDS0_TX2_N","LVDS","LVDS LCD"]
["S133","LCD_VDD_EN","Out","-","iMX6","EIM_A16","GPIO2_22","EIM1","CMOS / VDD_IO"]
["S134","LVDS0_CK+","Out","-","iMX6","LVDS0_CLK_P","LVDS0_CLK_P","LVDS","LVDS LCD"]
["S135","LVDS0_CK-","Out","-","iMX6","LVDS0_CLK_N","LVDS0_CLK_N","LVDS","LVDS LCD"]
["S136","GND","-","-","-","-","-",null,"-"]
["S137","LVDS0TX3+","Out","-","iMX6","LVDS0_TX3_P","LVDS0_TX3_P","LVDS","LVDS LCD"]
["S138","LVDS0TX3-","Out","-","iMX6","LVDS0_TX3_N","LVDS0_TX3_N","LVDS","LVDS LCD"]
["S139","I2C_LCD_CK","Out","PU-2k2","iMX6","KEY_COL3","SCL (I2C2)","GPIO","CMOS / VDD_IO"]
["S140","I2C_LCD_DAT","Bi-Dir","PU-2k2","iMX6","KEY_ROW3","SDA (I2C2)","GPIO","CMOS / VDD_IO"]
["S141","LCD_BKLT_PWM","Out","-","iMX6","SD1_DAT3","PWMO","SD1","CMOS / VDD_IO"]
["S142","LCD_DUAL_PCK","Out","-","FPGA","-","-",null,"CMOS / VDD_IO"]
["S143","GND","-","-","-","-","-",null,"-"]
["S144","RSVD / EDP_HPD","-","-","-","-","-",null,"RSVD"]
["S145","WDT_TIME_OUT#","Out","-","iMX6","GPIO_1","WDOG_B","GPIO","CMOS / VDD_IO"]
["S146","PCIE_WAKE#","In","W-PU","iMX6","EIM_DA10","GPIO3_10","EIM2+LS","CMOS 3.3V"]
["S147","VDD_RTC","PWR_IN","-","-","-","-",null,"PWR"]
["S148","LID#","In","W-PU","iMX6","GPIO_2","GPIO1-2","GPIO","CMOS / VDD_IO"]
["S149","SLEEP#","In","W-PU","iMX6","GPIO_4","GPIO1-4","GPIO","CMOS / VDD_IO"]
["S150","VIN_PWR_BAD#","In","W-PU","FPGA","-","-","+VDD_SNVS","CMOS / VDD_IO"]
["S151","CHARGING#","In","W-PU","iMX6","NANDF_RB0","GPIO1-18","SD1","CMOS / VDD_IO"]
["S152","CHARGER_PRSNT#","In","W-PU","iMX6","SD1_CLK","GPIO1-20","SD1","CMOS / VDD_IO"]
["S153","CARRIER_STBY#","Out","W-PU","iMX6","EIM_A25","GPIO5-2","EIM0","CMOS / VDD_IO"]
["S154","CARRIER_PON","Out","PD-10k","FPGA","-","-",null,"CMOS / VDD_IO"]
["S155","FORCE_RECOV#","In","W-PU","FPGA","-","-",null,"CMOS / VDD_IO"]
["S156","BATLOW#","In","W-PU","iMX6","SD1_DAT2","GPIO1-19","SD1","CMOS / VDD_IO"]
["S157","TEST#","In","W-PU","iMX6","GPIO_5","GPIO1-0","GPIO","CMOS / VDD_IO"]
["S158","VDD_IO_SEL#","Bi-Dir","-",null,"-","-",null,"Strap / VDD_IN"]
[]
["Internal Use Signals"]
[null,"EMMC_DAT0",null,null,"iMX6","SD4_DATA0","DAT0","SD4"]
[null,"EMMC_DAT1",null,null,"iMX6","SD4_DATA1","DAT1","SD4"]
[null,"EMMC_DAT2",null,null,"iMX6","SD4_DATA2","DAT2","SD4"]
[null,"EMMC_DAT3",null,null,"iMX6","SD4_DATA3","DAT3","SD4"]
[null,"EMMC_DAT4",null,null,"iMX6","SD4_DATA4","DAT4","SD4"]
[null,"EMMC_DAT5",null,null,"iMX6","SD4_DATA5","DAT5","SD4"]
[null,"EMMC_DAT6",null,null,"iMX6","SD4_DATA6","DAT6","SD4"]
[null,"EMMC_DAT7",null,null,"iMX6","SD4_DATA7","DAT7","SD4"]
[null,"EMMC_CK",null,null,"iMX6","SD4_CLK","CLK","SD4"]
[null,"EMMC_CMD",null,null,"iMX6","SD4_CMD","CMD","SD4"]
[null,"EMMC_RST#",null,null,"FPGA","RSM_RST#"]
[null,"I2C_FRAM_CK","Out",null,"iMX6","CSI0_DAT9","SCL (I2C1)"]
[null,"I2C_FRAM_DAT","Bi-Dir",null,"iMX6","CSI0_DAT8","SDA (I2C1)"]
[null,"I2C_PCIESW_CK","Out",null,"iMX6","CSI0_DAT9","SCL (I2C1)"]
[null,"I2C_PCIESW_DAT","Bi-Dir",null,"iMX6","CSI0_DAT8","SDA (I2C1)"]
[null,"I2C_PMIC_CK","Out",null,"iMX6","CSI0_DAT9","SCL (I2C1)"]
[null,"I2C_PMIC_DAT","Bi-Dir",null,"iMX6","CSI0_DAT8","SDA (I2C1)"]
[null,"VDD_IO_1.8#","In",null,"iMX6","EIM_DA15","GPIO3-15","EIM2","Low is 1.8V, high is 3.3V"]
[null,"PMIC_IRQ#","In",null,"iMX6","GPIO_18","GPIO7-13","GPIO"]
[]
[null,"W-PU is PU-100k"]
[]
[null,"重覆使用到 iMX6 Pins, Carrier board 必須避免同時使用."]
["S43","I2S1_LRCK","Bi-Dir","-","iMX6","DISP0_DAT22","AUD4_TXFS","LCD","CMOS / VDD_IO"]
["S44","I2S1_SDOUT","Out","-","iMX6","DISP0_DAT21","AUD4_TXD","LCD","CMOS / VDD_IO"]
["S45","I2S1_SDIN","In","-","iMX6","DISP0_DAT23","AUD4_RXD","LCD","CMOS / VDD_IO"]
["S46","I2S1_CK","Bi-Dir","-","iMX6","DISP0_DAT20","AUD4_TXC","LCD","CMOS / VDD_IO"]
["S115","LCD_D20","Out","-","iMX6","DISP0_DAT20 (I2S1)","LCD_D20","LCD","CMOS / VDD_IO"]
["S116","LCD_D21","Out","-","iMX6","DISP0_DAT21 (I2S1)","LCD_D21","LCD","CMOS / VDD_IO"]
["S117","LCD_D22","Out","-","iMX6","DISP0_DAT22 (I2S1)","LCD_D22","LCD","CMOS / VDD_IO"]
["S118","LCD_D23","Out","-","iMX6","DISP0_DAT23 (I2S1)","LCD_D23","LCD","CMOS / VDD_IO"]
["S50","I2S2_LRCK","Bi-Dir","-","iMX6","DISP0_DAT18","AUD5_TXFS","LCD","CMOS / VDD_IO"]
["S51","I2S2_SDOUT","Out","-","iMX6","DISP0_DAT17","AUD5_TXD","LCD","CMOS / VDD_IO"]
["S52","I2S2_SDIN","In","-","iMX6","DISP0_DAT19","AUD5_RXD","LCD","CMOS / VDD_IO"]
["S53","I2S2_CK","Bi-Dir","-","iMX6","DISP0_DAT16","AUD5_TXC","LCD","CMOS / VDD_IO"]
["S111","LCD_D16","Out","-","iMX6","DISP0_DAT16 (I2S2)","LCD_D16","LCD","CMOS / VDD_IO"]
["S112","LCD_D17","Out","-","iMX6","DISP0_DAT17 (I2S2)","LCD_D17","LCD","CMOS / VDD_IO"]
["S113","LCD_D18","Out","-","iMX6","DISP0_DAT18 (I2S2)","LCD_D18","LCD","CMOS / VDD_IO"]
["S114","LCD_D19","Out","-","iMX6","DISP0_DAT19 (I2S2)","LCD_D19","LCD","CMOS / VDD_IO"]
["S18","AFB1_OUT(MLB_DAT)","Bi-Dir","-","iMX6","GPIO_2","TBD","GPIO","CMOS / VDD_IO"]
["S148","LID#","In","W-PU","iMX6","GPIO_2","GPIO1-2","GPIO","CMOS / VDD_IO"]
["S17","AFB0_OUT(MLB_CLK)","Out","-","iMX6","GPIO_3","TBD","ENET+LS","CMOS / VDD_IO"]
["P77","PCIE_B_CKREQ#","In","PU-36k","iMX6","ENET_TXD1","GPIO1-29","ENET","CMOS 3.3V"]
["S19","AFB2_OUT(MLB_SIG)","Out","PU-2k2","iMX6","GPIO_6","TBD","GPIO","CMOS / VDD_IO"]
["P106","HDMI_CTRL_DAT","Bi-Dir","PU-2k2","iMX6","GPIO_6","SDA (I2C3)","GPIO","CMOS / VDD_IO"]
[]
[null,"+LS","為訊號有加 Level shift IC"]
[null,null,"Signal transfered by CPLD, will tri-state during iMX6 reset, drive to iMX6 after the end of iMX6 reset."]
["(*1)","SPDIF_IN function can not use for IEEE-1588 operation."]

{"sheet":"BootMode","index":2,"n_rows":11,"n_cols":19,"rows_kept":11,"cut":false,"hidden":false,"merged":[[0,2,0,4],[0,6,0,9],[0,17,0,18],[0,10,0,16]],"flags":["formulas_cached_only"]}
["Boot Function","FORCE_RECOV#","BOOT_SEL[2:0]#",null,null,"Boot Port","BOOT_CFG1_[7:4]",null,null,null,"BOOT_CFG2_[6:0]",{"$nulls":6},"Boot_Mode"]
[null,null,2,1,0,null,7,6,5,4,6,5,4,3,2,1,0,1,0]
["Carrier SATA",1,0,0,0,"SATA",0,0,1,0,0,0,1,0,0,0,1,1,0]
["Carrier SD card",1,0,0,1,"SDIO (4-bit)",0,1,0,0,0,1,0,1,0,0,0,1,0]
["Carrier eMMC",1,0,1,0,"SDMMC (8-bit)",0,1,1,0,1,0,1,0,0,0,0,1,0]
["Carrier SPI",1,0,1,1,"SPI1_CS0# (16-bit)",0,0,1,1,"z","z","z","z","z","z","z",1,0]
["Module Device (NAND NOR Flash)",1,1,0,0,"Not support","z","z","z","z","z","z","z","z","z","z","z",1,0]
["Module Serial Download",1,1,0,1,"Not support","z","z","z","z","z","z","z","z","z","z","z",1,0]
["Module eMMC",1,1,1,0,"EMMC (8-bit)",0,1,1,0,1,0,1,1,0,0,0,1,0]
["Module SPI",1,1,1,1,"Not support","z","z","z","z","z","z","z","z","z","z","z",1,0]
["Force Recovery",0,1,1,0,"USB0",0,0,1,1,0,0,0,0,0,0,0,0,1]